**ENGLISH TEMPLATE FOR TPDES or TLAP NEW/RENEWAL/AMENDMENT APPLICATIONS**

**DOMESTIC WASTEWATER**

*The following summary is provided for this pending water quality permit application being reviewed by the Texas Commission on Environmental Quality as required by 30 Texas Administrative Code Chapter 39. The information provided in this summary may change during the technical review of the application and are not federal enforceable representations of the permit application*.

LLIJ, LLC (CN606160414 ) operates the Brushy Creek Wastewater Treatment Plant RN111772463. an extended aeration activated sludge facility. The facility will be located at 6850 Farm-to-Market Road 973 North, in Williamson County, Texas 78615.

This application is for a new application to discharge at a daily average flow not to exceed 6,000 gallons per day.

Discharges from the facility are expected to contain five-day carbonaceous biochemical oxygen demand (CBOD5), total suspended solids (TSS), ammonia nitrogen (NH3-N), and *Escherichia coli*. Additional potential pollutants are included in the Domestic Technical Report 1.0, Section 7. Pollutant Analysis of Treated Effluent in the permit application package. Domestic wastewater will be treated byan extended aeration activated sludge process plant and the treatment units will include primary settling basins, equalization basins, aeration basins, final clarifiers, and a chlorine contact chamber.