**ENGLISH TEMPLATE FOR TPDES or TLAP NEW/RENEWAL/AMENDMENT APPLICATIONS**

**INDUSTRIAL WASTEWATER/STORMWATER**

*The following summary is provided for this pending water quality permit application being reviewed by the Texas Commission on Environmental Quality as required by 30 Texas Administrative Code Chapter 39. The information provided in this summary may change during the technical review of the application and are not federal enforceable representations of the permit application*.

Gulf Sulphur Services Ltd., LLC (CN600130181 ) operates Galveston Sulphur Terminal RN12911955. a solid and molten sulphur transfer facility. The facility is located at 4500 Old Port Industrial Road, in Galveston, Galveston County, Texas 77554.

This application is a renewal discharge process wastewater and stormwater on an intermittent and flow-variable basis from one outfall. <<*For TLAP applications include the following sentence, otherwise delete:>>* This permit will not authorize a discharge of pollutants into water in the state.

Discharges from the facility are expected to contain total suspended solids (TSS), chemical oxygen demand (COD), oil & grease, and total copper. Stormwater and process wastewater is treated bywith ferric sulfate and caustic to lower pH and remove copper prior to discharge.

**Example**

**Individual Industrial Wastewater Application**

*The following summary is provided for this pending water quality permit application being reviewed by the Texas Commission on Environmental Quality as required by 30 Texas Administrative Code Chapter 39. The information provided in this summary may change during the technical review of the application and are not federal enforceable representations of the permit application*.

ABC Corporation (CN600000000) operates the Starr Power Station (RN10000000000), a two-unit gas fired electric generating facility. Unit 1 has a generating capacity of 393 megawatts (MWs) and Unit 2 has a generating capacity of 528 MWs. The facility is located at 1356 Starr Street, near the City of Austin, Travis County, Texas 78753.

This application is for a renewal to discharge 870,000,000 gallons per day of once through cooling water, auxiliary cooling water, and also authorizes the following waste streams monitored inside the facility (internal outfalls) before it is mixed with the other wastewaters authorized for discharge via main Outfall 001, referred as “previously monitored effluents” (low volume wastewater, metal cleaning waste, and stormwater (from diked oil storage area yards, and storm drains)) via Outfall 001. Low volume waste sources, metal cleaning waste, and stormwater drains on a continuous and flow-variable basis via internal Outfall 101.

The discharge of once through cooling water via Outfall 001 and low volume waste and metal cleaning waste via Outfall 101 from this facility is subject to federal effluent limitation guidelines at 40 CFR Part 423. The pollutants expected from these discharges based on 40 CFR Part 423 are: free available chlorine, total residual chlorine, total suspended solids, oil and grease, total iron, total copper, and pH. Temperature is also expected from these discharges. Additional potential pollutants are included in the Industrial Wastewater Application Technical Report, Worksheet 2.0.

Cooling water and boiler make-up water are supplied by Lake Starr Reservoir. The City of Austin municipal water plant (CN600000000, PWS 00000) supplies the facility’s potable water and serves as an alternate source of boiler make-up water. Water from the Lake Starr Reservoir is withdrawn at the intake structure and treated with sodium hypochlorite to prevent biofouling and sodium bromide as a chlorine enhancer to improve efficacy and then passed through condensers and auxiliary equipment on a once-through basis to cool equipment and condense exhaust steam. Low volume wastewater from blowdown of boiler Units 1 and 2 and metal cleaning wastes receive no treatment prior to discharge via Outfall 101. Plant floor and equipment drains and stormwater runoff from diked oil storage areas, yards, and storm drains are routed through an oil and water separator prior to discharge via Outfall 101. Domestic wastewater, blowdown, and backwash water from the service water filter, clarifier, and sand filter are routed to the Starr Creek Domestic Sewage Treatment Plant, TPDES Permit No. WQ0010000001, for treatment and disposal. Metal cleaning waste from equipment cleaning is generally disposed of off-site.