**ENGLISH TEMPLATE FOR TPDES or TLAP NEW/RENEWAL/AMENDMENT APPLICATIONS**

**DOMESTIC WASTEWATER**

*The following summary is provided for this pending water quality permit application being reviewed by the Texas Commission on Environmental Quality as required by 30 Texas Administrative Code Chapter 39. The information provided in this summary may change during the technical review of the application and are not federal enforceable representations of the permit application*.

Eastwood Hills Mobile Home Park Limited Partnership, (CN600689863) operates Eastwood Hills Subdivision WWTF RN102183480, an wastewater treatment facility operated in extended aeration mode. The facility is located at 11315 Hillridge drive, Conroe, Montgomery County, Texas 77385.

This application is for renewal to discharge at an annual average flow of less than 50,000 gallons per day of treated domestic wastewater via Outfall 001.

Discharges from the facility are expected to contain five-day carbonaceous biochemical oxygen demand (CBOD5) total suspended solids (TSS), ammonia nitrogen (NH3-N) and *Escherichia coli.* Additional potential pollutants are included in the Domestic Technical Report 1.0, Section 7. Domestic wastewater is treated byextended aeration mode. Influent enters the aeration basin, then flows to the clarifier. Liquid then flows to chlorine contact chamber and after being in contact with the chlorine is discharged and solids flow to the digester.