Pine Cove Inc. (CN600677108) operates Pine Cove Crier Creek Wastewater Treatment Facility (RN105198109) at a youth camp. The facility is located 1123 Creekwood Lane, in Columbus, Colorado County, Texas 78934. This application is for a renewal and major modification to discharge at an annual flow of 80,000 gallons per day of treated domestic wastewater via Outfall 001.

Discharges from the facility are expected to contain five-day carbonaceous biochemical oxygen demand (CBOD5), total suspended solids (TSS), and *Escherichia coli*. Additional potential pollutants are included in the Domestic Technical Report 1.0, Section 7. Pollutant Analysis of Treated Effluent and Domestic Worksheet 4.0 in the permit application package. Domestic wastewater is treated bya sequencing batch reactor utilizing the activated sludge process followed by chlorine contact tank to disinfect the wastewater prior to discharge.