Section 15. Plain Language Summary (Instructions Page 40)

If you are subject to the alternative language notice requirements in [30 Texas Administrative Code §39.426](https://texreg.sos.state.tx.us/public/readtac%24ext.TacPage?sl=T&app=9&p_dir=N&p_rloc=66532&p_tloc=&p_ploc=1&pg=17&p_tac=&ti=30&pt=1&ch=39&rl=351), **you must provide a translated copy of the completed plain language summary in the appropriate alternative language as part of your application package**. For your convenience, a Spanish template has been provided below.

**ENGLISH TEMPLATE FOR TPDES or TLAP NEW/RENEWAL/AMENDMENT APPLICATIONS**

**DOMESTIC WASTEWATER**

*The following summary is provided for this pending water quality permit application being reviewed by the Texas Commission on Environmental Quality as required by 30 Texas Administrative Code Chapter 39. The information provided in this summary may change during the technical review of the application and are not federal enforceable representations of the permit application*.

Poetry Road MUD of Rockwall County (CN605782010 ) operates Poetry Village WWTP RN110295599. an extended aeration activated sludge TPDES facility. The facility is located approximately 992 feet (0.19 miles) northeast of the intersection of Pinon Trail and White Pine Dr., in Royse Coty, Rockwall County, Texas 75189.

This application is for a renewal to discharge at a daily average flow of 90,000 gallons per day of treated domestic wastewater.

Discharges from the facility are expected to containfive-day carbonaceous biochemical oxygen demand (CBOD5), total suspended solids (TSS), Escherichia Coli, and Ammonia Nitrogen. Additional pollutants are included in the Domestic Technical Report 1.0 in the permit application package.Domestic treated wastewater will be treated by *a bar screen, aeration basin, a clarifier, a digester and a chlorine contact chamber*.