**DOMESTIC WASTEWATER**

*The following summary is provided for this pending water quality permit application being reviewed by the Texas Commission on Environmental Quality as required by 30 Texas Administrative Code Chapter 39. The information provided in this summary may change during the technical review of the application and are not federal enforceable representations of the permit application*.

TA Operating LLC (CN603171661 ) operates Petro Stopping Center 340 RN111506051. a gas station and truck stop. The facility is located 101 North Cornelius Road, in Carl’s Corner, Hill County, Texas 76645.

This application is for a new application to authorize the discharge of treated wastewater at a volume not to exceed a daily average flow of 45,000 gallons per day.

Discharges from the facility are expected to contain biochemical oxygen demand, total suspended solids, E. coli and dissolved oxygen. Sewage is treated byrouting it to equalization chamber, thence to a flow splitter, thence to one of two prepackaged extended aeration systems. In each prepackaged system, sewage passes through a bar screen to an aeration chamber and then to a clarifying chamber. Sludge is transferred to a digester and effluent is moved to a chlorine chamber, and then piped to the discharge point. The first prepackaged system is 15,000-gallons, and the second system is 30,000-gallons.