**ENGLISH TEMPLATE FOR TPDES or TLAP NEW/RENEWAL/AMENDMENT APPLICATIONS**

**DOMESTIC WASTEWATER**

*The following summary is provided for this pending water quality permit application being reviewed by the Texas Commission on Environmental Quality as required by 30 Texas Administrative Code Chapter 39. The information provided in this summary may change during the technical review of the application and are not federal enforceable representations of the permit application*.

Terrell Timmermann Farms, LP (CN606063709 ) proposes to operate Kelly Farm Wastewater Treatment Plant RN111579082. an activated sludge domestic wastewater treatment plant. The facility will be located 12995 East Highway 29, in Georgetown, Williamson County, Texas 78626.

This application is for a new authorization to discharge treated wastewater at a volume not to exceed a daily average flow of 975,000 gallons per day.

Discharges from the facility are expected to contain five-day carbonaceous biochemical oxygen demand (CBOD5), Total Suspended Solids (TSS), Ammonia Nitrogen (NH3-N), and Escherichia coli. Domestic Wastewater will be treated by *an activated sludge process plant and the treatment units include: a bar screen, aeration basins, clarifiers, chlorine contact basins (or UV disinfection), effluent filters, and sludge holding basins*.